{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Liste de débit","Devis"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Liste de débit","index":0,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[[5,9,8,9],[1,9,2,9],[10,9,21,9],[24,9,38,9],[0,8,0,9],[24,0,38,0],[10,8,14,8],[10,7,14,7],[17,7,21,7],[17,8,21,8],[24,7,26,7],[24,8,26,8],[29,7,30,7],[29,8,30,8],[33,8,34,8],[33,7,34,7],[37,7,38,7],[37,8,38,8],[10,0,21,0],[1,8,2,8],[5,0,8,0],[1,0,2,0]]}
["Section Comiale","Désignation","Qt","larg.","Haut","Long.","Long. +","Lg Cm","Qt Lg Cm"]
["30 x 190","Bandeau droit",4,21,180,2.5230000000000001,{"$f":"F2+0.15","v":2.673},5.5,null,4]
[null,"Bandeau gch",4,21,180,2.5230000000000001,{"$f":"F3+0.15","v":2.673},5.5]
[null,null,4,null,null,null,5.4]
[]
["60 x 170","Entrait 1/2 ferme",4,50,160,2.0569999999999999,{"$f":"F6+0.15","v":2.2069999999999999},5,{"$f":"Repart(G6,H6,C6)","v":2},4]
[null,null,2,null,null,null,4.4000000000000004]
[]
[null,"Entrait",2,50,160,4.4000000000000004,{"$f":"F9+0.15","v":4.5500000000000007},5,{"$f":"Repart(G9,H6,C9)","v":2}]
[]
["70 x 90","Chevron droit",4,60,80,1.546,{"$f":"F11+0.1","v":1.6460000000000001},5.5,{"$f":"Repart(G11+G12+G13+G14+G15,H11,C11)","v":4},8]
[null,"Empan. brisis droit",4,60,80,0.60699999999999998,{"$f":"F12+0.1","v":0.70699999999999996}]
[null,"Empan. court droit",4,60,80,0.47099999999999997,{"$f":"F13+0.1","v":0.57099999999999995}]
[null,"Empan. long droit",4,60,80,1.3959999999999999,{"$f":"F14+0.1","v":1.496}]
[null,"Empan. moyen droit",4,60,80,0.93400000000000005,{"$f":"F15+0.1","v":1.034}]
[null,null,4,null,null,null,{"$f":"G11+G12+G13+G14+G15","v":5.4539999999999997}]
[]
[null,"Chevron gch",4,60,80,1.546,{"$f":"F18+0.1","v":1.6460000000000001},5.5,{"$f":"Repart(G18+G19+G20+G21+G22,H18,C18)","v":4}]
[null,"Empan. brisis gch",4,60,80,0.60699999999999998,{"$f":"F19+0.1","v":0.70699999999999996}]
[null,"Empan. court gch",4,60,80,0.47099999999999997,{"$f":"F20+0.1","v":0.57099999999999995}]
[null,"Empan. long gch",4,60,80,1.3959999999999999,{"$f":"F21+0.1","v":1.496}]
[null,"Empan. moyen gch",4,60,80,0.93400000000000005,{"$f":"F22+0.1","v":1.034}]
[null,null,4,null,null,null,{"$f":"G18+G19+G20+G21+G22","v":5.4539999999999997}]
[]
["100 x 190","Fourrure coyau",4,90,127,2.5760000000000001,{"$f":"F25+0.15","v":2.726},5.5,{"$f":"Repart(G25+G26+G27,H25,C25)","v":4},14]
[null,"1/2 panne haute",4,80,180,1.2549999999999999,{"$f":"F26+0.15","v":1.4049999999999998}]
[null,"Panne brisis",4,80,180,1.214,{"$f":"F27+0.15","v":1.3639999999999999}]
[null,null,4,null,null,null,{"$f":"G27+G26+G25","v":5.4949999999999992}]
[]
[null,"Panne porteuse",4,80,180,3.2589999999999999,{"$f":"F30+0.15","v":3.4089999999999998},5.5,{"$f":"Repart(G30+G31,H30,C30)","v":4}]
[null,"1/2 panne basse",4,80,180,1.9850000000000001,{"$f":"F31+0.15","v":2.1350000000000002}]
[null,null,4,null,null,null,{"$f":"G30+G31","v":5.5440000000000005}]
[]
[null,"Coyau",4,90,160,2.093,{"$f":"F34+0.15","v":2.2429999999999999},5.5,{"$f":"Repart(G34+G35,H34,C34)","v":4}]
[null,"Arbalétrier",4,90,180,2.7290000000000001,{"$f":"F35+0.15","v":2.879}]
[null,null,4,null,null,null,{"$f":"G34+G35","v":5.1219999999999999}]
[]
[null,"Fourrure arba",4,90,145,1.34,{"$f":"F38+0.15","v":1.49},5.5,{"$f":"Repart(G38+G39,H38,C38)","v":2}]
[null,"Contrefiche",4,70,120,0.79400000000000004,{"$f":"F39+0.15","v":0.94400000000000006}]
[null,null,4,null,null,null,{"$f":"G39+G38","v":2.4340000000000002}]
[]
["170 x 170","Poinçon",1,160,160,1.3420000000000001,{"$f":"F42+0.15","v":1.492},3,null,1]
[]
["210 x 210","Poteau",4,200,200,2.698,{"$f":"F44+0.15","v":2.8479999999999999},3,null,4]
[]
[null,"Semelle",2,50,160,0.4,{"$f":"F46+0.15","v":0.55000000000000004},3,null,1]

{"sheet":"Devis","index":1,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,5,1,5],[0,7,1,7],[0,1,0,2],[0,3,1,3],[0,4,1,4],[0,6,1,6]]}
["Désignation","section ",null,"Lg","Qt.","Vol.","P.U HT","Montant HT"]
[null,"Hauteur","Largeur"]
[null,"  [mm]","[mm]","[m]","[u]","[m3]","[€/m3]","[€]"]
["Douglas",30,190,5.5,4,{"$f":"E4*D4*C4*B4/1000000","v":0.12540000000000001},580,{"$f":"G4*F4","v":72.732000000000014}]
["Douglas",60,170,5,4,{"$f":"E5*D5*C5*B5/1000000","v":0.20399999999999999},580,{"$f":"G5*F5","v":118.32}]
["Douglas",70,90,5.5,8,{"$f":"E6*D6*C6*B6/1000000","v":0.2772},580,{"$f":"G6*F6","v":160.77600000000001}]
["Douglas",100,190,5.5,14,{"$f":"E7*D7*C7*B7/1000000","v":1.4630000000000001},550,{"$f":"G7*F7","v":804.65000000000009}]
["Douglas",170,170,3,1,{"$f":"E8*D8*C8*B8/1000000","v":8.6699999999999999E-2},550,{"$f":"G8*F8","v":47.685000000000002}]
["Douglas",210,210,3,4,{"$f":"E9*D9*C9*B9/1000000","v":0.5292},550,{"$f":"G9*F9","v":291.06}]
[]
["Transport",null,null,null,1,null,null,100]
[]
["Bois de charpente, brut de sciage, vive arête"]
[]
[null,null,null,null,null,null,"Volume total [m3]",{"$f":"F8+F9+F7+F5+F4+F6","v":2.6855000000000002}]
[null,null,null,null,null,null,"Total H.T.",{"$f":"H8+H9+H7+H5+H4+H6","v":1495.223}]
[null,null,null,null,null,null,"Total T.V.A.",{"$f":"H16*0.196","v":293.06370800000002}]
[null,null,null,null,null,null,"Net à payer",{"$f":"H16+H17","v":1788.2867080000001}]